**New Lshell commands for C-390 \KC-390 HOLAND- Embraer**

The commands are case-sensitive.

|  |  |  |
| --- | --- | --- |
| **Directory** | **Command** | **Description** |
| LaserTech | Command:  **zc**  parameters:  Choose one!  **0**- Do nothing  **1**- Zeroize CUST tech | The command zeroized the Cust techniques After the Zeroize is completed, the system will be rebooted. |
| LaserTech | Command:  **zo**  parameters:  Choose one!  **0**- Do nothing  **1**- Delete OEM tech | The command Delete the OEM techniques After the deletion is completed, the system will be rebooted. |
| LaserTech | Command:  **u**  parameters:  All of them needed!  Tech Type – **s**(sw)/**l**(lw)  File num – **0**/**1**  Tech Path - ***c:\tech\swc.dat*** | The command uploads the CUST technique to the Safe. |
| LaserTech | Command:  **d**  parameters:  None | The command copies the techniques from Safe to the ramDisk and allows receiving a success indication of the upload (**u**)command. |
| ltec | Command:  **jc**  parameters:  Choose one!  **No parameters** – Print Current JC only.  **0** – Change JC to OEM  **1** – Change JC to CUST | After executing the command, the selection will be saved in the SelectedJammingCode.ini file. A system reboot will then be triggered. |